|  | | | **型式の区分** (Type Classification) | | --- | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | **特 定 電 気 用 品 名**  (Name of Specified Electrical Appliance and Material) | | **:** | | アンペア制用電流制限器 (Meter rate current limiters) | |
|  | | **要　素** (Factor) | | **区　分** (Classification) | |
|  | | 相及び線式 (Phase and wiring type) | | (1) 単相２線式のもの (Single phase, two wire type)  (2) 単相３線式のもの (Single phase, three wire type)  (3) その他のもの (Others) | |
|  | | 定格電圧 (Rated voltage) | | (1) 125Ｖ以下のもの (125V or less)  (2) 125Ｖを超えるもの (Exceeding 125V) | |
|  | | 定格電流 (Rated current) | | (1) ５Ａ以下のもの (5A or less)  (2) ５Ａを超え7.5Ａ以下のもの (Exceeding 5A, and less than or equal to 7.5A)  (3) 7.5Ａを超え10Ａ以下のもの (Exceeding 7.5A, and less than or equal to 10A)  (4) 10Ａを超え15Ａ以下のもの (Exceeding 10A, and less than or equal to 15A)  (5) 15Ａを超え20Ａ以下のもの (Exceeding 15A, and less than or equal to 20A)  (6) 20Ａを超え25Ａ以下のもの (Exceeding 20A, and less than or equal to 25A)  (7) 25Ａを超え30Ａ以下のもの (Exceeding 25A, and less than or equal to 30A)  (8) 30Ａを超え40Ａ以下のもの (Exceeding 30A, and less than or equal to 40A)  (9) 40Ａを超え50Ａ以下のもの (Exceeding 40A, and less than or equal to 50A)  (10) 50Ａを超え60Ａ以下のもの (Exceeding 50A, and less than or equal to 60A)  (11) 60Ａを超えるもの (Exceeding 60A) | |
|  | | 極 (Poles) | | (1) 単極のもの (Single poles)  (2) ２極のもの (Two poles)  (3) ３極以上のもの (Three or more poles) | |
|  | | 接続する電線の種類 (Type of cable or cord to be connected) | | (1) 銅のもの (Copper)  (2) その他のもの (Others) | |
|  | | 過電流引き外し素子の数 (Number of over current tripping elements) | | (1) １のもの (One)  (2) ２以上のもの (Two or more) | |
|  | | 過電流引き外し機構 (Overcurrent tripping mechanism) | | (1) 熱動式のもの (Thermal type)  (2) 電磁式のもの (Electromagnetic type)  (3) その他のもの (Others) | |
|  | | 接点の材料 (Contact materials) | | (1) 銀のもの又は銀合金のもの (Silver or silver alloy)  (2) 銅のもの又は銅合金のもの (Copper or copper alloy)  (3) その他のもの (Others) | |
|  | | 開閉操作の方式 (Switching operation) | | (1) タンブラー式のもの (Tumbler type)  (2) 押しボタン式のもの (Push button type)  (3) 引きひも式のもの (Pull cord type)  (4) その他のもの (Others) | |
|  | | 外郭の材料 (Outer case materials) | | (1) 金属のもの (Metal)  (2) 合成樹脂のもの (Plastic)  (3) その他のもの (Others) | |
|  | | 使用場所 (Place for use) | | (1) 屋外のもの (Outdoors)  (2) 屋内のもの (Indoors) | |
|  | | 定格遮断電流 (Rated breaking capacity) | | (1) 1,000Ａ以下のもの (1,000A or less)  (2) 1,000Ａを超え1,500Ａ以下のもの (Exceeding 1,000A, and less than or equal to 1,500A)  (3) 1,500Ａを超え2,500Ａ以下のもの (Exceeding 1,500A, and less than or equal to 2,500A)  (4) 2,500Ａを超え5,000Ａ以下のもの (Exceeding 2,500A, and less than or equal to 5,000A)  (5) 5,000Ａを超え7,500Ａ以下のもの (Exceeding 5,000A, and less than or equal to 7,500A)  (6) 7,500Ａを超え10,000Ａ以下のもの (Exceeding 7,500A, and less than or equal to 10,000A)  (7) 10,000Ａを超え15,000Ａ以下のもの (Exceeding 10,000A, and less than or equal to 15,000A)  (8) 15,000Ａを超え20,000Ａ以下のもの (Exceeding 15,000A, and less than or equal to 20,000A)  (9) 20,000Ａを超え25,000Ａ以下のもの (Exceeding 20,000A, and less than or equal to 25,000A)  (10) 25,000Ａを超え30,000Ａ以下のもの (Exceeding 25,000A, and less than or equal to 30,000A)  (11) 30,000Ａを超えるもの (Exceeding 30,000A) | |