|  |

| **型式の区分** (Type Classification) |
| --- |

 |
| --- | --- | --- |
|  | **特 定 電 気 用 品 名**(Name of Specified Electrical Appliance and Material) | **:** | 温度ヒューズ (Thermal fuses) |
|  | **要　素** (Factor) | **区　分** (Classification) |
|  | 定格電圧 (Rated voltage) | [ ]  (1) 125Ｖ以下のもの (125V or less)[ ]  (2) 125Ｖを超えるもの (Exceeding 125V) |
|  | 定格電流 (Rated current) | [ ]  (1) ５Ａ以下のもの (5A or less)[ ]  (2) ５Ａを超え15Ａ以下のもの (Exceeding 5A, and less than or equal to 15A)[ ]  (3) 15Ａを超え30Ａ以下のもの (Exceeding 15A, and less than or equal to 30A)[ ]  (1) 30Ａを超えるもの (Exceeding 30A) |
|  | 公称動作温度 (Nominal operating temperature) | [ ]  (1) 80℃以下のもの (80℃ or less)[ ]  (2) 80℃を超え100℃以下のもの (Exceeding 80℃, and less than or equal to 100℃)[ ]  (3) 100℃を超え120℃以下のもの (Exceeding 100℃, and less than or equal to 120℃)[ ]  (4) 120℃を超え140℃以下のもの (Exceeding 120℃, and less than or equal to 140℃)[ ]  (5) 140℃を超え160℃以下のもの (Exceeding 140℃, and less than or equal to 160℃)[ ]  (6) 160℃を超え180℃以下のもの (Exceeding 160℃, and less than or equal to 180℃)[ ]  (7) 180℃を超え200℃以下のもの (Exceeding 180℃, and less than or equal to 200℃)[ ]  (8) 200℃を超え220℃以下のもの (Exceeding 200℃, and less than or equal to 220℃)[ ]  (9) 220℃を超え240℃以下のもの (Exceeding 220℃, and less than or equal to 240℃)[ ]  (10) 240℃を超え260℃以下のもの (Exceeding 240℃, and less than or equal to 260℃)[ ]  (11) 260℃を超え280℃以下のもの (Exceeding 260℃, and less than or equal to 280℃)[ ]  (12) 280℃を超え300℃以下のもの (Exceeding 280℃, and less than or equal to 300℃)[ ]  (13) 300℃を超えるもの (Exceeding 300℃) |
|  | 可溶体への通電 (Current to fuse element) | [ ]  (1) あるもの (Yes)[ ]  (2) ないもの (No) |
|  | 可溶体の主材料 (Fuse element materials) | [ ]  (1) すず、鉛及びビスマスの合金のもの (Tin, lead, and bismuth alloy)[ ]  (2) すず、鉛及びビスマスの合金以外の合金のもの (Alloy other than tin, lead, and bismuth alloy)[ ]  (3) 合成樹脂又は有機化合物のもの (Plastic or organic compound)[ ]  (4) その他のもの (Others) |
|  | 容器 (Container) | [ ]  (1) あるもの (With container)[ ]  (2) ないもの (Without container) |
|  | 端子 (Terminals) | [ ]  (1) つめ形（丸形を含む。）のもの (Fork tongue terminals (including ring tongue terminals.))[ ]  (2) 線付きのもの (Wire lead)[ ]  (3) その他のもの (Others) |
|  | 可溶体の形状 (Shape of fuse element) | [ ]  (1) 板状のもの (Plate)[ ]  (2) 塊状のもの (Block)[ ]  (3) その他もの (Others) |